Customer Quality Drivers CTQ necessity

Requirements

Must have an accuracy of ±2 mmHg.

Accuracy

Quality

products

High reliability with minimum failure rate.

Reliability

Must comply with relevant safety standards.

User friendly

interface

Safety

Quick

Application

Should be made for easy to use during high stress environment.

Easy to operate & handle.

Clear results

Must be compatible with various age groups & arm sizes.

Compatibility

Sterile

packaging

Packaging

Must provide adequate protection during storage & transportation.